TN-19-00-001 January 24, 2019	Tesla, Inc. Tech Notes
Model: All	Vehicle System: 00 - Inspection & Service	Region: Australia

Vehicle Pre-Delivery and Inspection (PDI) Process

Tech Notes are announcements that help to communicate and track new information about Tesla Service concerns. Such concerns may or may not be VIN specific. These instructions assume knowledge of motor vehicle and high voltage electrical component repairs, and should only be executed by trained professionals. Tesla assumes no liability for injury or property damage due to a failure to properly follow these instructions or for repairs attempted by unqualified individuals.

Fill out this form within 24 hours of a vehicle arriving at the delivery location. Email the completed form to one of the following locations:

VIC:	DL-AU-MelbournePDI@tesla.com

NSW:	DL-AU-SydneyPDI@tesla.com

QLD:	DL-AU-BrisbanePDI@tesla.com

Date: Click or tap to enter a date.	Delivery Location:
VIN: Last Six	Model: Choose an item.	Odometer:
Inspected by:	Signature:

Vehicle OK ☐
Additional Work Required ☐ If additional repairs are required, write them in this area.

Receiving	☐ Remove the transport cover/vehicle wrap and exterior plastics. Report any damage that might have occurred during transport or unwrapping within 24 hours.
Visual Inspection Accessories Supplied in Vehicle	☐ All glass for chips or cracks ☐ All exterior panels for damage (scratches, dents, chips, etc.) ☐ All tyres are OK (bulges, cuts, nails) ☐ Wheels are OK (No paint defects or damage) ☐ Use a tyre pressure gauge to make sure that the tyre pressures are at the correct PSI (see tyre placard). ☐ Floor mats ☐ Cup holders ☐ License plate bracket(s) ☐ 1 X 10 amp adapter and charge cables ☐ Tow hook ☐ Phone dock kit (if applicable)
Functional Inspection	☐ Remove the vehicle from Transport mode. ☐ Both keys/access cards are present and working. ☐ Charge port door ☐ All interior and exterior lights ☐ Windshield wipers ☐ Make sure that the washer fluid is full. ☐ HVAC system. Ensure that air conditioning blows cold air without noise. ☐ All moving glass (check for operation and noise). ☐ All doors (front, rear, and trunk). Ensure they unlock or open with a key and from the touchscreen, and then ensure all closures are closed. ☐ Seats. Fold the rear seats down and up, making sure that they are secure. ☐ Seat controls. Cycle each control one time. Make sure that the seats have a full range of motion. ☐ Seatbelts. Firmly tug on the buckle and lower seat anchors. Extract the belt fully, and tug the seat belt from the B-pillar, making sure that the retractor is attached. Ensure seat belts retract into the stow position. ☐ Glove box: Opens and closes smoothly. ☐ Ensure that Australian Quick Guide is in the glove box. Remove all other documents. ☐ Ensure that all radio and connectivity functions for the region operate correctly, if equipped: FM, Spotify, Satellite Radio, Internet, Wi-Fi, GPS. ☐ Check that all wheel nuts are torqued to 175 Nm.
Special Check Items	☐ Model S only: Perform a functional check of door handles. ☐ Model X only: Perform a functional check of the rear doors. ☐ Model 3 only: Remove the protective plastic on the touch screen. ☐ Model 3 only: Make sure that the USB cables are in the rear center console.
Final Inspection	☐ Leave the protective interior plastic fitted to the sill panels. ☐ Make sure that the vehicle does not display any malfunction indicators. ☐ Visually inspect all seats, interior trim, and roof for staining or damage. ☐ Return the vehicle to Transport mode. ☐ Attach a green “COMPLETE” sticker to the right hand top of the windscreen.

.